**SMCP AND SLOT-KIT**

**TILT CODE REFERENCE SERIES 142**

|  |  |  |
| --- | --- | --- |
| CODE | DESCRIPTION | DIRECTIONS |
| -0- | INTERNAL COIN COUNT METERS ERASED | CHECK NICAD BATTERY AND/OR POWER SUPPLY |
| -1- | COIN-IN JAM, SELF CLEARED | CHECK COIN PATH, THEN PUSH HOPPER RESET AND CONTINUE |
| -2- | COIN-IN SWITCH JAM | CLEAR JAM, CHECK COIN PATH, THEN CONTINUE |
| X3- | REEL X SPINNIN SLOW | PULL HANDLE FOR REPLAY, NOTIFY MAINTENANCE IF EXCESSIVE REPEATS |
| X4- | REEL X SPINNING BACKWARD |
| X5- | CANNOT READ REEL X WHILE SPINNING |
| X6- | REEL X FAILED TO STOP |
| X7- | REEL X OVER SPEED |
| X-Y | REEL X INDEXED EARLY BY Y STOPS | PULL HANDLE FOR REPLAY, NOTIFY MAINTENANCE IF EXCESSIVE REPEATS |
| X-Y | REEL X INDEXED LATE BY Y STOPS |
| -8- | COIN-OUT SWITCH JAM | CLEAR JAM, CHECK COIN PATH, HOPPER RST, PAYOUT CONTINUES WHEN DOOR CLOSES |
| -9- | COIN-OUT JAM, SELF CLEARED | CHECK COIN PATH, PUSH HOPPER RESET, PAYOUT CONTINUES WHEN DOOR CLOSES |
| --- | EXTRA COINS PAID OUT | NOTIFY MAINTENANCE, PUSH MASTER RESET TO RETURN GAME TO PLAY |
| --- | FREE HANDLE PULL, SELF CLEARED | CHECK HANDLE RELEASE AND/OR HANDLE MECH, NOTIFY MAINTENANCE |