|  |
| --- |
| Summit Systems Win-Meter Code Reference Chart  |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **SMCP ANDS SLOT-KIT****WIN-METER CODE REFERENCE SERIES 142****METER READOUT:**OPERATE JACKPOT RESET SWITCH (ON SIDE OF MACHINE), ELECTRONIC METERS WILL DISPLAY IN 3 STEPS**METER CODE** **............ METER VALUE**

|  |  |  |
| --- | --- | --- |
| Meter  | Thousands  | Hundreds  |
| X  | N N N  | N N N  |
| First Display  | Second Display  | Third Display  |

**METER CODE** **VALUE**1. 1..................................TOTAL COIN-IN
2. 2..................................TOTAL COIN-OUT (MACHINE PAID)
3. 3..................................TOTAL COIN DROP
4. 4..................................TOTAL HANDLE PULLS
5. 5..................................TOTAL COIN HAND PAID (J/P)
6. 6..................................HOPPER LEVEL VARIANCE, COINS
7. OVER OR UNDER THE REQUIRED FILL
8. 7..................................CURRENT HOPPER COIN COUNT

**WIN-METER FLASHING:** HOPPER EMPTY OR NOT PICKING UP COINS**TIME-OUT IF COINS REMAIN:** CLEAR PICK-UP PROBLEM, PUSH HOPPER RESET, PAYOUT RESUMES WHEN DOOR IS CLOSED**EMPTY IF NO COINS REMAIN:** FILL HOPPER, PUSH HOPPER FILL, PAYOUT RESUMES WHEN DOOR IS CLOSED |