|  |
| --- |
| Summit Systems Win-Meter Code Reference Chart |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **SMCP ANDS SLOT-KIT**  **WIN-METER CODE REFERENCE SERIES 142**  **METER READOUT:**  OPERATE JACKPOT RESET SWITCH (ON SIDE OF MACHINE), ELECTRONIC METERS WILL DISPLAY IN 3 STEPS  **METER CODE** **............ METER VALUE**   |  |  |  | | --- | --- | --- | | Meter | Thousands | Hundreds | | X | N N N | N N N | | First Display | Second Display | Third Display |   **METER CODE** **VALUE**   1. 1..................................TOTAL COIN-IN 2. 2..................................TOTAL COIN-OUT (MACHINE PAID) 3. 3..................................TOTAL COIN DROP 4. 4..................................TOTAL HANDLE PULLS 5. 5..................................TOTAL COIN HAND PAID (J/P) 6. 6..................................HOPPER LEVEL VARIANCE, COINS 7. OVER OR UNDER THE REQUIRED FILL 8. 7..................................CURRENT HOPPER COIN COUNT   **WIN-METER FLASHING:** HOPPER EMPTY OR NOT PICKING UP COINS  **TIME-OUT IF COINS REMAIN:** CLEAR PICK-UP PROBLEM, PUSH HOPPER RESET, PAYOUT RESUMES WHEN DOOR IS CLOSED  **EMPTY IF NO COINS REMAIN:** FILL HOPPER, PUSH HOPPER FILL, PAYOUT RESUMES WHEN DOOR IS CLOSED |